

***NEWS RELEASE****Editor’s note: Hi-res photo available upon request*

Media Contact:
Carolyn Schinsky / Ryan PR / 314-822-9784/ carolyn@ryan-pr.com

**Touch ‘n Seal Announces New In-Line Chemical Filter**

**for CPDS Spray Foam Dispensing System Hose Sets**

*Filter Improves Delivery of Spray Foam Insulation, Reduces Waste*



ST. LOUIS—Aug. 27, 2012— Convenience Products, the manufacturer of [Touch ‘n Seal Insulating Foams and Sealants](http://www.touch-n-seal.com), announces a new, in-line chemical filter designed for use with Touch ‘n Seal’s [CPDS Series 2](http://touch-n-seal.com/constantpressuresprayfoam.htm) Spray Foam Dispensing System chemical hose sets.  The CPDS, one of the company’s top-rated specialty products, uses an internal air compressor to deliver higher spray foam yield at more than twice the speed as foam kits.

“The new filter improves spray foam delivery by preventing any hardened particles in the chemical hoses from clogging the CPDS spray foam applicator, which in turn increases the life of the applicator and helps ensure consistent quality of the spray foam,” says Michael Sites, Touch ‘n Seal Marketing Manager.  “The filter also helps reduce waste of usable spray foam if partially used chemical sets are not stored in the proper temperature range.”

The lightweight in-line filter is easy-to-install, reusable and can be easily disassembled for cleaning with Touch ‘n Seal’s zero VOC [Poly-Clean](http://touch-n-seal.com/polyclean.htm) polyurethane foam cleaner.

The in-line filter comes preinstalled on the “A” side chemical hose that comes with the CPDS Series 2 unit. The chemical filter can be used on both the “A” and “B” side chemical hoses if desired. The chemical filter can be ordered separately (item number 4505500170) and retrofitted to CPDS 100’ and 150’ hose sets and all existing CPDS spray foam hoses.

To place an order, contact your local distributor contact or Touch ‘n Seal’s customer care department at (800) 325-6180, ext. 1.

# # #

**About Touch ‘n Seal**

Convenience Products, the manufacturer of Touch ‘n Seal products, is headquartered in St. Louis, Missouri. Touch ‘n Seal insulating foams and sealants are the benchmark for performance in commercial and industrial building and maintenance, OEM manufacturing and specialty applications. A full line of one and two-component spray foams and adhesives are available, including fire blocking foam  (ICC-ES: ESR-1926), Low Pressure Window & Door Foam, Drywall Panel Adhesives, Heating Systems and Accessories, Two-Component, Disposable Units, Mining Specialty Units and One-Component Disposable Cylinders. Spray foam is available from 15-board feet kits to 120-gallon refill systems.  One-component straw and gun foam available in 12 to 30.5 oz. aerosol cans. More information is available at [www.touch-n-seal.com](http://www.touch-n-seal.com), [www.facebook.com/TouchNSeal](http://www.facebook.com/TouchNSeal) and [www.twitter.com/TouchNSeal](http://www.twitter.com/TouchNSeal).